                Avance Logic AC'97 Sound System Software        ver: A3.13
                        Installation and Setup


Driver & Application Installation/Removal Procedure For Avance AC'97 Codec:
=================================================================================

<<< For Win98/Win2000/WinME (WDM driver) >>>

---------------------------------------
Setup Driver/Application at first time:
---------------------------------------

Step 1. Before installing the Avance AC'97 Drivers & Applications, Press the
        [Cancel] button if Windows detect the PCI Multimedia Audio device. 
          
Step 2. Insert the "Avance AC'97 Drivers & Applications" CD into the CD-ROM 
        drive and run the setup.exe program to finish the installation. 

Step 3. Click on [Next/OK/Go] to continue the procedure. If the Windows popup 
        "Digital Signature Not Found" message, press [Yes] to continue the 
        installation.
        
Step 4. Finally, select to restart the system and press [Finish] to complete
        the installation.  

        The system will reload the drivers and do some adjustments in the INF
        file if so required.

--------------------------
Update Driver/Application:
--------------------------

Step 1. Follow Step 2,3,4 described in [Setup at first time] above to complete
        the procedure.

--------------------------
Remove Driver/Application:
--------------------------

Step 1. Go to Start\Settings\Control Panel.

Step 2. Select [Add/Remove Programs] icon.

Step 3. Select "Avance AC'97 Drivers and Applications" and press [Change/Remove]
        button.

Step 4. Click on [Next/OK/Go] to finish the uninstallation.        

Step 5. At the end of the procedure, select to restart the system and press
        [Finish] to complete the uninstallation.


<<< For WinNT 4.0 (NT4 driver) >>>

---------------------------------------
Setup Driver/Application at first time:
---------------------------------------

    Ignore Step 1, and follow the same procedure in Win98.

--------------------------
Update Driver/Application:
--------------------------

    The same procedure in Win98.
    
--------------------------
Remove Driver/Application:
--------------------------

    The same procedure in Win98.

--------------------
Silent Installation:
--------------------

Run "Setup -s -f2<path\LogFile>"
i.e. setup -s -f2c:\mylog.log 


Note: AVRack only works fine under WinNT 4.0 after installing
      Service Pick 3 or later.


---------------------
Version Informations:
---------------------

WDM driver for Win98SE/WinMe/Win2000/WinXP : 5.10.0.3850
VXD driver for Win95/Win98Gold             : 4.5.0.3017
VXD Software wavetable driver              : 3.1.0.0
NT4 driver for Windows NT4                 : 4.3.0.3027
NT4 software wavetable driver              : 4.3.0.2001

AvRack for Win98/Me/2000                   : 2002.4.3.0
AvRack for Win95/NT4                       : 2002.4.3.1

Avance Sound Effect Manager                : 5.0.0.0
Avance Sound Effect Manager for NT4        : 2.3

Driver/Application Setup Program           : 4.70

--------
History:
--------
A3.13 - compare to A2.73
1. To avoid mapping lost on Win98SE by raising IRQ level and adding TagCount before get mappings.
2. Disable "Phone Line" for some specific models.
3. Improve S/W SRC (if needed) quality to meet PC99 requirement.
4. Mute SPDIF while master volume was muted.
5. Improve EAX 1.0 compatible issue.

A2.73 -
1.  First release for ALC202A.
2.  The drivers in this package has passed logo for ALC202A.
