## System Summary

The Show System Summary screen displays basic information about the access point's current configuration such as the unit name, IP address, MAC address, and ESSID. This screen also provided information about the current firmware version and the serial number of the unit.

### Web Interface

- Select System Properties from the Statistics Menu at the left side of the screen.

### Management Console

- Select Show System Summary from the Main Menu. Press ESC to return to the previous menu

### Parameter Descriptions

Unit Name | Identifies the access point name.
MAC Address (BSS) | Identifies the unique 48-bit, hard-coded Media Access Control address.
IP Address | Identifies the network-assigned Internet Protocol address.
Net_ID (ESS) | Identifies the unique 32-character, alphanumeric, case-sensitive network identifier.
Channel | Identifies the direct-sequence channel used by the access point. The channel used is within the range required for the operating country.
Country | Identifies access point country code that in turn determines the access point direct-sequence channel range.
Antenna Selection | Indicates if the access point is configured for single or dual antenna mode.
WEP (Privacy) | Defines the WEP algorithm. Admin privileges are required to make changes to this parameter. The default is Disabled .
WEP Algorithm | Defines the number of bits and type of WEP algorithm used. Admin privileges are required to make changes to this parameter. The default is 40 bit shared .
Current MUs | Specifies the current number of associated clients.
Total Assoc | Specifies the total client associations handled by this access point.
System Up Time | Specifies how long the system has been operational. System Up Time resets to zero after 119,304 hours.
Access Control | Specifies if the access control feature is enabled or disabled. If enabled, the ACL specifies the MAC addresses of the clients that can associate with this access point.
WLAP Mode | Specifies if wireless access point operation status is enabled. If enabled, the access point sets up automatically for wireless operation. This feature is Disabled by default.
Model Number | Identifies the model number.
Serial Number | States the access points unique identifier.
Hardware Revision | Specifies the hardware version.
AP Firmware Ver | Specifies the firmware version.
RF Firmware Ver | Specifies the Radio firmware version.
HTML File Ver | Specifies the HTML file version.
Start Flashing All LEDs | Begins a test routine to check the LED functionality and allows you to determine the access point location.
Reset AP | Clears the access points statistics and restores the last saved configuration.

Copyright © 2002 Intel Corporation. Legal Information