Chips and Technologies, Inc.
Release Notes
65548/548 PCI Display Driver Package
OS/2

These drivers function with the  65545,65546 and 65548 
video controllers on PCI Bus only.

Revision:      4.1.0
Release Date:  August 23, 1996
=============================


  1.  Initial release of drivers which use INT 10 enabled VDD and
      BVH, and provide Multiple Refresh support.


Revision:      4.1.1
Release Date:  September 18, 1996
===============================

  1.  Fixed problem with video corruption when DOS Window is started.

  
Revision:      4.2.0
Release Date:  October  07, 1996
===============================

  1.  Fixed problem starting WIN-OS2 Full Screen session in Background.
  
  2.  Switch to default LCD resolution when starting CRT Only resolution in 
      LCD environment ( No CRT attached ) has been modified to corrrectly
      update Windows SYSTEM.INI settings.
      
  
