














Normally, your computer should have enabled the adapter for
busmaster operation during power-up.  This server didn't.

The adapter Setup program and drivers take care of this
problem for you in most cases.

However, if you have problems with your adapter failing
diagnostic tests, move the adapter to another slot in your
server and try the test again.

If you still have problems, contact your network services
supplier.
