# Adapter Specifications

Feature | Value
--- | ---
PCI bus compatibility | PCI 2.2 specification
Connector | RJ-45, 100BASE-TX
Power requirements | 1.06 watts @ +5VDC
Interrupt | INTA
LEDs | Two: Link/Activity, 100 Mbps
Duplex mode | Half or Full duplex
Data Rate | 10 or 100 Mbps
Transmit/Receive Buffer | 6 Kbytes
Dimensions | TBD
Weight | TBD
Operating temperature | 32 - 131 deg. F (0 - 55 C)
Humidity | 10% - 90%, non-condensing
Standards conformance | IEEE 802.3 IEEE 802.3ac IEEE 802.3z IEEE 802.3x IEEE 802.1p IEEE 802.1Q PCI 2.2 specification
Compliance & Certification | UL, FCC Class B, CE & Immunity, Ctick (Australia)
Included Software | Intel PROSet configuration and diagnostics utility Intel Boot Agent Intel Priority Packet Intel Teaming (Servers only)