Intel(R) PRO/100 Server Adapter and Desktop Adapter Supplemental Information
November 10, 2000
============================================================================


Browser-Viewable Online User's Guide
====================================

The PRO/100 adapter User's Guide is viewable with any recent web 
browser. To view the guide, start the Windows Explorer, go to 
the \INFO folder in this archive and double-click the file called 
INDEX.HTM.

If you do not have a browser installed, you can obtain one from:

	Netscape:    http://www.netscape.com
	Microsoft:   http://www.microsoft.com
	Opera:       http://www.opera.com


Installing PROSet II and Other Advanced Features
================================================

To install PROSet II, run the batch file INSTALL_PROSET.BAT in the
root directory of this archive.

      NOTE: In Windows NT 4.0, Intel PROSet II is automatically
      pre-installed when you install the adapter drivers.

      For Windows 95, only Intel(R) PROSet is available.

Other tools and advanced features are available from support.intel.com
in the following archives;

100PDMI2.EXE  - Desktop Management Interface 
100PWMI.EXE   - Intel(R) PRO Network Adapters WMI Provider 
100PWMI.EXE   - Intel(R) PRO Quality of Service WMI Provider 
PRTPKT2.EXE   - Intel(R) Priority Packet II 
100PCSI.EXE   - Intel(R) Common Software Installer
100PBOOT.EXE  - Intel(R) Boot Agent tools

Each of these archives includes individual installation and use
instructions. They all require the driver set in this download except
for 100PBOOT.EXE.

Alternatively, you can download 100PCSI.EXE and use the Intel(R) Common
Software Installer to manage the installation process of all installable
components. The Intel(R) Common Software Installer is an installation
utility that can be used to install the following Advanced Features:

  - Intel(R) PROSet II
  - Desktop Management Interface 
  - Intel(R) PRO Network Adapters WMI Provider 
  - Intel(R) PRO Quality of Service WMI Provider 
  - Intel(R) Priority Packet II 

See the file RELNOTES.TXT under the heading of "Additional Software" for
instructions on how to recreate the original CD contents and use the Common
Software Installer.
      
Server Adapter Teaming Features
===============================

Server adapters support advanced teaming features:

   Adapter Fault Tolerance (AFT)
   Adaptive Load Balancing (ALB)
   Fast EtherChannel* (FEC)
   802.3ad

For more information on these teaming features and how to set up
teaming on specific adapters, see the Online User's Guide.


VLANS on PRO/100 Adapters
=========================

A VLAN is a logical grouping of network devices put together as a LAN 
regardless of their physical grouping or collision domains. VLANs let a user 
see and access only specified network segments. This optimizes network 
efficiency and maintains security access restrictions. VLANs require special 
switches that are capable of supporting VLANs. PRO/100 adapters support VLANs
when attached to a VLAN-enabled switch. 

A VLAN offers you the ability to group users and client PCs together into 
logical workgroups, a critical consideration when connecting clients to 
servers that are geographically dispersed across the building, campus, or 
enterprise network.

Typically, VLANs consist of a common set of coworkers within the same 
department but in different locations, a cross-functional team working on a 
joint project, or a diverse set of users sharing the same network 
application. Joining workers across the network forms logical working groups.
By using VLANs on your network, you can:

  - Improve network performance
  - Limit broadcast storms
  - Improve adds, moves, and changes
  - Minimize security problems
  - Ease your management task

For overview information on Intel VLANs, visit the Intel Networking Web site: 

   http://www.intel.com/network

For more specific information, read the white paper on VLANs:

   http://www.intel.com/network/tech_brief/virtual_lans.htm


Making Floppy Disks for NetWare and Windows Installation
========================================================

If you need to use a floppy disk to install the adapter 
drivers, use the MAKEDISK.BAT utility located in the 
\MAKEDISK directory on this CD.

MAKEDISK [operating system] [destination]

where [operating system] is the OS for which you are creating the
diskette, and [destination] is the drive letter and path (such
as A:). If no destination is specified, the A: drive will be used.

The possible [operating system] options are:

NT    = Microsoft Windows NT
W2K   = Microsoft Windows* 2000
W9X   = Microsoft Windows* 95 and Windows 98 and Windows* ME
NW    = Novell NetWare servers and clients
DOS   = Microsoft DOS and IBM OS2
MODEM = Modem drivers for the PRO/100 Mobile Combo adapters
        for all Microsoft operating systems.

Make sure you have a 1.44 MB formatted, non-bootable diskette in
the floppy drive when using this utility.

NOTE: Due to size limitations, PROSet and other advanced features
      cannot be installed from the floppy disk.

NOTE: This utility MUST be run from the \MAKEDISK directory.


      Alternately, you can use the following .BAT files (located
      in the \MAKEDISK directory on this CD) to simplify this process:

      MAKEW9X.BAT -- Creates a drivers disk for Windows 95 and
                     Windows 98.

      MAKENT.BAT  -- Creates drivers disks for Windows NT.

      MAKEW2K.BAT -- Creates a drivers disk for Windows 2000.
 
      MAKENW.BAT  -- Creates a drivers disk for Novell NetWare
                     servers and clients.


Management Adapters
===================

For more information on the Management adapters, see the 
MANAGEMENT Topic in the Online User's Guide.


DMI and SNMP Software Support
=============================

This adapter provides Desktop Management Interface 2.0 and SNMP
capability for your Management applications. Software for DMI and
SNMP is located in the \dmi-snmp directory in this archive.

For DMI-SNMP information for NetWare, see the dminet.txt file in the 
\dmi-snmp\snmp\nwserver directory.

For DMI-SNMP information for Windows NT, see the dmiwin.txt file in the 
\dmi-snmp\snmp\win32 directory.


Push Installations
==================

If you are a network administrator interested in unattended installation
of the adapter drivers (push installation), see the Online User's Guide.


Updating Software and Drivers in Windows 98
===========================================

If you're using Windows 98 and have updated or added an adapter,
you may experience a problem with device driver update files not being
copied.  (This is a known problem, for which Microsoft has published a
Knowledge Base article, Q242150.)

To resolve this problem, perform the following:

1. Reboot the computer.

2. Remove the adapter via Device Manager and reboot the computer again.

3. When prompted for the adapter driver, choose the option "Display a
   list of all the drivers...".  Then choose the adapter from the list
   and click Have Disk to update the drivers from this archive.

4. Reboot the computer.


Removing Adapter Drivers in Windows 98 and Windows 2000
=======================================================

If you use the Add/Remove Programs icon in the Windows Control Panel
to remove an Intel adapter, and then try to install drivers from a later
Intel driver release, you may see a prompt asking for the following files:

"Prodd.vxd"
"Prokddp.vxd"

This is because Windows is attempting to install the files associated
with the earlier driver, which are not present in the later drivers.

To resolve this problem, finish the installation and choose "Skip" when
prompted for a missing file.  Then, instead of removing the driver,
update it with the later Intel drivers.

For instructions on updating the adapter driver, see the "Install the
Network Drivers" section in the online guide in this archive. (For
instructions on viewing the online guide, see the section
"Browser-Viewable Online User's Guide," earlier in this readme.

For instructions on installing PROSet II, see the section 
"Installing PROSet II and Other Advanced Features," earlier in this
readme.


Web-Based Enterprise Management (WBEM) Applications and Windows 98
==================================================================

On Windows 98 operating systems you must carefully configure
client systems to allow remote access of Intel network adapters
WMI provider properties.

To do this, you will need to edit the Windows 98 registry to 
remotely access the adapters WMI provider properties on Windows 98
systems from Windows NT. 

Refer to the Readme.txt file in \WBEM\WMI\NIC or \WBEM\WMI\QOS in the
archive 100PWMI.EXE.


Known Limitations and Compatibility Notes
=========================================

This section contains a list of notes that are not documented in the
online guides or otherwise described.


Network Adapter Flash Memory Information Not Accessible
-------------------------------------------------------

Normally Intel PROSet can read the flash memory of each Intel adapter in
your computer. This functionality will not be available if you install
any dual port adapter in the same computer, such as the Intel PRO/100 
Dual Port Server Adapter. The Boot Agent tab in PROSet will not be visible
when a dual port adapter is installed. There is no workaround for this 
condition at this time.


Windows Millennium Edition
--------------------------

If you plan to install a new Intel adapter in a computer while also installing 
Windows Me, see the special installation notes in the Online User's Guide. Go 
to the "Installing the Network Drivers" section and click the Windows Me link.









*  Third party trademarks or brand names are the property of their owners.
